(footprint "TP_2P_Keystone_1430-2"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -2.54 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "71372c38-847e-421e-b7ee-5b7454e44864")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "TT_nP_fp_value_mgr-pn"
		(at 0 -6.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "b92d6e19-a091-456b-9fdb-5e0a70cd2f4c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5ab55a21-f937-4c15-a03d-a8af4acbe57a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b27b7bfd-bc2f-4e16-a50d-e1707f528a15")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "61fd50a5-620a-4855-a268-c734c624926e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -5.08 0.635)
		(end -5.08 -0.635)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "8d26a547-3504-4049-9bb9-d54a9ab36fe2")
	)
	(fp_line
		(start -3.81 -1.905)
		(end 3.81 -1.905)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a8aa1a39-47c1-4491-a3cc-187eab8b15f5")
	)
	(fp_line
		(start 3.81 1.905)
		(end -3.81 1.905)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c7600a1f-4869-45f0-8d9e-446283a694f3")
	)
	(fp_line
		(start 5.08 -0.635)
		(end 5.08 0.635)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "dc6a45f8-68e8-441c-9157-61e6758992fc")
	)
	(fp_arc
		(start -5.08 -0.635)
		(mid -4.708026 -1.533026)
		(end -3.81 -1.905)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b8664cf5-dddc-4580-82ce-b6af1ac5bf25")
	)
	(fp_arc
		(start -3.81 1.905)
		(mid -4.708026 1.533026)
		(end -5.08 0.635)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "71d3d71a-fdd3-44e6-ad9b-8b741e90ca07")
	)
	(fp_arc
		(start 3.81 -1.905)
		(mid 4.708026 -1.533026)
		(end 5.08 -0.635)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "9fe82dc9-a6b0-4893-bafa-2cf612b07ee8")
	)
	(fp_arc
		(start 5.08 0.635)
		(mid 4.708026 1.533026)
		(end 3.81 1.905)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "8859f645-9ad0-42b5-909d-1bb8d497be47")
	)
	(fp_rect
		(start -5.08 -1.905)
		(end 5.08 1.905)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "5d54ac1d-ba88-4b08-b9cf-00b9d65e0923")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "bdd70080-2682-4c7c-bf8d-dd829a8539e0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at -3.175 0)
		(size 2.54 2.54)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "93d73754-ab97-48db-a552-5479b1a128f4")
	)
	(pad "2" thru_hole circle
		(at 3.175 0)
		(size 2.54 2.54)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "296882be-7699-49eb-bb34-6e9187efe139")
	)
	(model "${KICAD_DDCEE_TEMPLATE_DIR}/mCAD/1430-2.STEP"
		(offset
			(xyz -3.175 0 -1.6)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
