(footprint "CN_40P_PPPC202LFBN-RC"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 20.574 3.302 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "71372c38-847e-421e-b7ee-5b7454e44864")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "CN_40P_PPPC202LFBN-RC"
		(at -15.494 -3.81 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b92d6e19-a091-456b-9fdb-5e0a70cd2f4c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at -24.13 -1.27 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5ab55a21-f937-4c15-a03d-a8af4acbe57a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at -24.13 -1.27 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b27b7bfd-bc2f-4e16-a50d-e1707f528a15")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at -24.13 -1.27 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "61fd50a5-620a-4855-a268-c734c624926e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_rect
		(start -25.65 -2.54)
		(end 25.65 2.54)
		(stroke
			(width 0.2)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "f14c67cc-b35d-4cfd-a749-c86807a84d36")
	)
	(fp_poly
		(pts
			(xy 24.13 2.794) (xy 23.368 3.81) (xy 24.892 3.81)
		)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "979a7756-e9e4-4e96-9e79-569c97d37db0")
	)
	(fp_rect
		(start -25.654 -2.54)
		(end 25.654 2.54)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "621c0696-db55-445e-b566-8369bec8c3ec")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "bdd70080-2682-4c7c-bf8d-dd829a8539e0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 24.13 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
		(uuid "0acea205-4ca6-47c6-82f6-d225fd24d85c")
	)
	(pad "2" thru_hole circle
		(at 24.13 -1.27)
		(size 1.76 1.76)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "99a1f2ca-829f-45d8-95d6-47b4aca7ad2a")
	)
	(pad "3" thru_hole circle
		(at 21.59 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d6595968-bd23-4f04-aac6-6ee0a4926d74")
	)
	(pad "4" thru_hole circle
		(at 21.59 -1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8495c3aa-a042-4d6e-a3d6-132d71198a91")
	)
	(pad "5" thru_hole circle
		(at 19.05 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5d4b29af-ad7e-432c-b2a1-e1c04cd1c8bb")
	)
	(pad "6" thru_hole circle
		(at 19.05 -1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3d31b6e2-72e2-417b-a24a-518bca4ae234")
	)
	(pad "7" thru_hole circle
		(at 16.51 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "51d23ccd-202c-4403-9c6f-d8c5e5a4482a")
	)
	(pad "8" thru_hole circle
		(at 16.51 -1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "cf9038f3-8456-4acb-8e20-36b83dd8a1eb")
	)
	(pad "9" thru_hole circle
		(at 13.97 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "975533b4-abaf-413f-851b-f08aefe569f3")
	)
	(pad "10" thru_hole circle
		(at 13.97 -1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2b164878-129c-4384-9ed7-5dabae636f55")
	)
	(pad "11" thru_hole circle
		(at 11.43 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ceaf355e-6d01-4801-8c04-f0e2a733c204")
	)
	(pad "12" thru_hole circle
		(at 11.43 -1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "55b2f81c-989e-4807-8b64-f72735c6b25a")
	)
	(pad "13" thru_hole circle
		(at 8.89 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "32cf710d-aa46-4cfd-b6e2-ac8e30404b1f")
	)
	(pad "14" thru_hole circle
		(at 8.89 -1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "19b7154d-5c4d-4352-bb64-51a73412a212")
	)
	(pad "15" thru_hole circle
		(at 6.35 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9055a797-c433-4665-84e6-37c37cecda54")
	)
	(pad "16" thru_hole circle
		(at 6.35 -1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2225cf44-ec4c-43c2-bb94-887a28c71809")
	)
	(pad "17" thru_hole circle
		(at 3.81 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4438a6bc-261e-4877-904f-342cd26354ef")
	)
	(pad "18" thru_hole circle
		(at 3.81 -1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "42f4222d-2ec7-483f-836f-8f3be2ad0163")
	)
	(pad "19" thru_hole circle
		(at 1.27 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ed232c47-28c3-4d10-bc7e-c65a0bf40d61")
	)
	(pad "20" thru_hole circle
		(at 1.27 -1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "11926818-537d-4c72-a527-1275cb07299c")
	)
	(pad "21" thru_hole circle
		(at -1.27 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "40f200ee-22d1-493e-a420-60a7358798fd")
	)
	(pad "22" thru_hole circle
		(at -1.27 -1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9462f584-f7b7-4090-8949-1688152a174e")
	)
	(pad "23" thru_hole circle
		(at -3.81 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "49758eaa-0c1b-41ec-8f8f-7a838dce3b80")
	)
	(pad "24" thru_hole circle
		(at -3.81 -1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "373e6ebd-fdf4-4508-bd88-5ee5324d747f")
	)
	(pad "25" thru_hole circle
		(at -6.35 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2b1d5668-8e7f-45aa-a8e1-375aff4b9652")
	)
	(pad "26" thru_hole circle
		(at -6.35 -1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a8a55f15-7caa-40ec-ae10-2ac1d55e85d3")
	)
	(pad "27" thru_hole circle
		(at -8.89 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fe842fe9-e7d6-4565-9aa4-65ca3fa40522")
	)
	(pad "28" thru_hole circle
		(at -8.89 -1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "eed70f14-80c4-4226-ac54-80aadce633c1")
	)
	(pad "29" thru_hole circle
		(at -11.43 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "afbadb64-1b4a-4d52-aa2f-84e2b9d6df3c")
	)
	(pad "30" thru_hole circle
		(at -11.43 -1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "56f56cfd-76c6-4121-9b11-d6087c7e38a6")
	)
	(pad "31" thru_hole circle
		(at -13.97 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "67589c1d-9941-4f67-bb15-8ce50411a0d0")
	)
	(pad "32" thru_hole circle
		(at -13.97 -1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "16b66de9-6d7b-438f-8bc0-40861c8042cd")
	)
	(pad "33" thru_hole circle
		(at -16.51 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "159f817e-be80-4619-b5ac-6738da94bc2c")
	)
	(pad "34" thru_hole circle
		(at -16.51 -1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "dae3fc13-c01d-4d11-ab35-254ea2a6a92f")
	)
	(pad "35" thru_hole circle
		(at -19.05 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f73f452e-f04b-4f54-ba08-e117bae5830e")
	)
	(pad "36" thru_hole circle
		(at -19.05 -1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4921a84c-40a5-4fa9-96e9-b58c7c9c48ee")
	)
	(pad "37" thru_hole circle
		(at -21.59 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "41497d6a-1b18-4b20-a6e6-06f4faa61265")
	)
	(pad "38" thru_hole circle
		(at -21.59 -1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5ffeb06f-c8fa-437e-b1de-40709e986228")
	)
	(pad "39" thru_hole circle
		(at -24.13 1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9658038f-d53a-4121-8ed7-69b2aaf2d7e5")
	)
	(pad "40" thru_hole circle
		(at -24.13 -1.27)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "265fb899-b157-40d1-a3f5-09bd5a8c2fc3")
	)
	(model "${KICAD_DDCEE_TEMPLATE_DIR}/mCAD/PPPC202LFBN-RC.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
